[Info] MAC: 00:80:e1:00:00:55
[Info] Found PHY at Address 1 (ID: 0007 c0f1)
[Info] Resetting PHY at address 1...
[Debug] Hardware abstraction layer initialized

[Info] Main: OSAL Log Level = 4

[Info] Test osal_log_i from main
[Debug] Initializing application components...

[Info] Event queue initialized
[Debug] Event queue initialized

[Info] Event handler initialized
[Debug] Event handler initialized

[Info] Transaction management initialized
[Debug] Transaction management initialized

[Info] State manager initialized
[Debug] State manager initialized

[Info] Error handler initialized
[Debug] Error handler initialized

[Info] Event handler registered for type 1
[Info] Event handler registered for type 2
[Info] Event handler registered for type 3
[Info] Event handler registered for type 4
[Info] Event handler registered for type 5
[Info] Event handler registered for type 7
[Info] Event handler registered for type 8
[Debug] Event handlers registered

[Debug] Initializing network components...

[Debug] Initializing TCP/IP stack...

[Debug] TCP/IP stack initialized.

[Debug] Network interface added

[Debug] Initializing sensors...

[Info] SHT40: Sending reset command 0x89
[Info] SHT40: Reset successful
[Info] SHT40 sensor initialized successfully
[Info] Sensor state set to 2
[Info] Performing SHT40 self-calibration using heater...
[Info] SHT40 self-calibration completed successfully
[Debug] Creating threads...

[Debug] Thread 'event_dispatch' created.

[Debug] Thread 'net_mon' created.

[Debug] Thread 'eth_input' created.

[Debug] Thread 'tcp_server' created.

[Debug] Thread 'blink' created.

[Debug] Memory Info: Total=88720, Used=12192, MaxUsed=12192

[Debug] System initialization completed. Starting OSAL...

[Info] Starting DHCP...
[Info] PHY BSR=0x7809, LinkStatus=0
.[Info] PHY BSR=0x782d, LinkStatus=1
[Info] Ethernet Link Up
[Info] Network link is up, starting DHCP...

[Info] Ethernet Link Down
.[Info] PHY BSR=0x782d, LinkStatus=1
[Info] Ethernet Link Up
.[Info] PHY BSR=0x782d, LinkStatus=1
.[Info] PHY BSR=0x782d, LinkStatus=1
.[Info] PHY BSR=0x782d, LinkStatus=1
.[Info] PHY BSR=0x782d, LinkStatus=1
.[Info] PHY BSR=0x782d, LinkStatus=1
.[Info] PHY BSR=0x782d, LinkStatus=1
.[Info] PHY BSR=0x782d, LinkStatus=1
.[Info] PHY BSR=0x782d, LinkStatus=1
.[Info] PHY BSR=0x782d, LinkStatus=1
.[Info] PHY BSR=0x782d, LinkStatus=1
.[Info] PHY BSR=0x782d, LinkStatus=1
.[Info] PHY BSR=0x782d, LinkStatus=1
.[Info] PHY BSR=0x782d, LinkStatus=1
.[Info] PHY BSR=0x782d, LinkStatus=1
.[Info] PHY BSR=0x782d, LinkStatus=1
.[Info] PHY BSR=0x782d, LinkStatus=1
.[Info] PHY BSR=0x782d, LinkStatus=1
.[Info] PHY BSR=0x782d, LinkStatus=1
.[Info] PHY BSR=0x782d, LinkStatus=1
.[Info] PHY BSR=0x782d, LinkStatus=1
.[Info] PHY BSR=0x782d, LinkStatus=1
.[Info] PHY BSR=0x782d, LinkStatus=1
.[Info] PHY BSR=0x782d, LinkStatus=1
.[Info] PHY BSR=0x782d, LinkStatus=1
.[Info] PHY BSR=0x782d, LinkStatus=1
.[Info] PHY BSR=0x782d, LinkStatus=1
.[Info] PHY BSR=0x782d, LinkStatus=1
.[Info] PHY BSR=0x782d, LinkStatus=1
.
[Warning] DHCP Timeout! Fallback to Static IP.
[Debug] Processing event type 2
[Info] Handling network connected event
[Info] Network state set to 2
[Info] IP Address: 192.168.1.10
[Info] Netmask:    255.255.255.0
[Info] Gateway:    192.168.1.1
[Info] PHY BSR=0x782d, LinkStatus=1
[Info] TCP Server Starting...
[Info] TCP Server listening on port 5588
[Info] PHY BSR=0x782d, LinkStatus=1
[Info] PHY BSR=0x782d, LinkStatus=1
[Info] PHY BSR=0x782d, LinkStatus=1
[Info] PHY BSR=0x782d, LinkStatus=1
[Info] PHY BSR=0x782d, LinkStatus=1
[Info] PHY BSR=0x782d, LinkStatus=1
[Info] PHY BSR=0x782d, LinkStatus=1
[Info] PHY BSR=0x782d, LinkStatus=1
[Info] PHY BSR=0x782d, LinkStatus=1
[Info] PHY BSR=0x782d, LinkStatus=1
[Info] PHY BSR=0x782d, LinkStatus=1
